MCKEE 510 KNEEBOARD M5 Multisystem

Front fins @ 15” from tail

Back fins @ 9-1/2” from tail

Distance between the back fins 7”

Fin direction @ fronts  2-7/8” from stringer at nose.

                     @ backs 7/8”      “         “         “     “

Tri fin tail fin @ 7-1/2”
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